BIOS History For Foxconn
==============================================================================
Model :	P55A01			FAB : A		Author : Cyril Wu
Old version : 
New version : 934F1D01.BIN	Code Base : 02/20/2009	Build date : 03/10/2009

LAN ROM	  : 
Raid BIOS : 
CheckSum  : 8E9E (h)
Description for Customer :
	1.First Release BIOS Debug Version.
==============================================================================
Model :	P55A01			FAB : A		Author : Arcer Hwang
Old version : 934F1D01.BIN
New version : 934F1D02.BIN	Code Base : 02/20/2009	Build date : 04/03/2009

LAN ROM	  : 
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 411E (h)
Description for Customer :
	1. Added "Debug Code Control" item.(Cyril Wu)
	2. Added Audio Verb. table.(Cyril Wu)
	3. Added "VIA 6308S 1394 Device" item.
	4. Added "Realtek 8111D LAN 1" item.
	5. Added "Realtek 8111D LAN 2" item.
	6. Added "Marvell 6121 PATA and eSATA" item.
==============================================================================
Model :	P55A01			FAB : A		Author : Arcer Hwang
Old version : 934F1D02.BIN
New version : 934F1D03.BIN	Code Base : 02/20/2009	Build date : 05/06/2009

LAN ROM	  : 
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : DB5B (h)
Description for Customer :
	1. Added Hardware Monitor page.
	2. Fixed USB Key Board can't work.
	3. Modify BIOS CMOS setup screen for Quantum BIOS.
	4. Added support PCIE 8x 8x.
	5. Fixed S3 resume Marvell IDE port device disappear.
	6. Added PS2 Key Board wake-up function.
	7. Added Power Loss Recover function.
	8. Update Lynnfield MRC to version 0.8.
	9. Update Havendale MRC to version 0.62.
==============================================================================
Model :	P55A01			FAB : A		Author : Arcer Hwang
Old version : 934F1D03.BIN
New version : 934F1D04.BIN	Code Base : 02/20/2009	Build date : 06/15/2009

LAN ROM	  : 
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : CFEF (h)
Description for Customer :
	1. Modify BIOS for CMOS lost default date from 2002/01/01 to BIOS build date.
	2. Fixed S1 state power LED can't blinking.
	3. Fixed CPU core show from "1" to "4" if Lynnfiled CPU present.
	4. Fixed can't show onboard LAN MAC address.
	5. Fixed "CPU Ratio" item no function.
	6. Fixed S4 Resume function abnormal issue.
	7. Update Lynnfield MRC to version 0.9.
	8. Update Havendale MRC to version 0.63.
	9. Update AMI BIOS Piketon platform to version 007.
	10.Update AMI BIOS Piketon platform NB code to version 016.
	11.Update AMI BIOS Piketon platform PCH code to version 020.
	12.Update Intel ignition firmware to version 1110.
	13.Modify BIOS ROM size from 1M Byte to 2M Byte for Intel ignition firmware.
==============================================================================
Model :	P55A01			FAB : A		Author : Arcer Hwang
Old version : 934F1D04.BIN
New version : 934F1D05.BIN	Code Base : 02/20/2009	Build date : 06/17/2009

LAN ROM	  : 
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 4D3D (h)
Description for Customer :
	1. Fixed S1 state power LED can't blinking(D04 still failed).
==============================================================================
Model :	P55A01			FAB : B		Author : Arcer Hwang
Old version : 979F1D05.BIN
New version : 979F1D06.BIN(2MB)	Code Base : 02/20/2009	Build date : 07/23/2009
New version : 979F1D06.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : E005 (h) 979F1D06.BIN
CheckSum  : 7F93 (h) 979F1D06.ROM
Description for Customer :
	1. Update Intel Raid ROM to version 8.9.0.1023.
	2. Update Intel Ignition firmware to version 6.0.0.1126.
	3. Update Lynnfield MRC to version 1.10.
	4. Update Havendale MRC to version 0.70.
	5. Update AMI BIOS Piketon platform NB code to version 021.
	6. Update AMI BIOS Piketon platform PCH code to version 025.
	7. Fixed Hot reset and reset bottom issue.
	8. Added OC Gear feature.
	9. Added Over Voltage feature.
	10.Added Over Clock feature.
	11.Added Over memory ratio feature.
	12.Added support SLI.
	13.Fixed ATI CrossFireX can't work issue.
	14.Modify for some string show.
	15.Creat Q.F. BIOS items.
==============================================================================
Model :	P55A01			FAB : B		Author : Arcer Hwang
Old version : 979F1D06.BIN
New version : 979F1D07.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/04/2009
New version : 979F1D07.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 3AA6(h) 979F1D07.BIN
CheckSum  : DA34(h) 979F1D07.ROM
Description for Customer :
	1. Added LAN Boot ROM control item.
	2. Modify PCH's LPC PME GPIO from GPI6 to GPI8.
	3. Update AMI BIOS Piketon platform NB code to version 023.
	4. Update AMI BIOS Piketon platform PCH code to version 026.
	5. Update AMI BIOS Piketon platform CPU code to version 01.06.
==============================================================================
Model :	P55A01			FAB : B		Author : Arcer Hwang
Old version : 979F1D07.BIN, 979F1D07.ROM
New version : 979F1D08.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/10/2009
New version : 979F1D08.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : FEFF(h) 979F1D08.BIN
CheckSum  : 9E8D(h) 979F1D08.ROM
Description for Customer :
	1. Fixed OC Gear function failed when use USB keyboard.
==============================================================================
Model :	P55A01			FAB : 1.0	Author : Arcer Hwang
Old version : 979F1D08.BIN, 979F1D08.ROM
New version : 979F1D09.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/12/2009
New version : 979F1D09.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 7871(h) 979F1D08.BIN
CheckSum  : 17FF(h) 979F1D08.ROM
Description for Customer :
	1. Fixed recovery card issue.
	2. Fixed sometime hang-up at BIOS POST code D3h.
	3. Fixed memory size show wrong with Clarkdale CPU.
==============================================================================
Model :	P55A01			FAB : 1.0	Author : Arcer Hwang
Old version : 979F1D09.BIN, 979F1D09.ROM
New version : 979F1P01.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/12/2009
New version : 979F1P01.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 981C(h) 979F1P01.BIN
CheckSum  : 37B5(h) 979F1P01.ROM
Description for Customer :
	1. First release P version.
==============================================================================
Model :	P55A01			FAB : 1.0	Author : Arcer Hwang
Old version : 979F1P01.BIN, 979F1P01.ROM
New version : 979F1D10.BIN(2MB)	Code Base : 02/20/2009	Build date : 08/21/2009
New version : 979F1D10.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 36AD(h) 979F1D10.BIN
CheckSum  : D646(h) 979F1D10.ROM
Description for Customer :
	1. Update AMI BIOS Piketon platform NB code to version 024.
	2. Update AMI BIOS Piketon platform PCH code to version 030.
	3. Update AMI BIOS Intel PPM DT code to version 02.00.
	4. Update Intel Lynnfield and Clarkdale CPU microcode as bellow :
	   M13106E5_00000003.TXT,M1320651_FFFF000F.TXT,M1320652_FFFF0008.TXT.
	5. Added Support OC Recovery feature.
==============================================================================
Model :	P55A01			FAB : 1.0		Author : Arcer Hwang
Old version : 979F1D10.BIN, 979F1P02.ROM
New version : 979F1P02.BIN(2MB)	Code Base : 02/20/2009	Build date : 09/03/2009
New version : 979F1P02.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 4847(h) 979F1P02.BIN
CheckSum  : E7E0(h) 979F1P02.ROM
Description for Customer :
	1. Removed DMI type 3 information.
	2. Modify DMI Slot information.
==============================================================================
Model :	P55A01			FAB : 1.0		Author : Arcer Hwang
Old version : 979F1P02.BIN, 979F1P02.ROM
New version : 979F1P03.BIN(2MB)	Code Base : 02/20/2009	Build date : 09/17/2009
New version : 979F1P03.ROM(1MB)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 9AD2(h) 979F1P03.BIN
CheckSum  : 3A6B(h) 979F1P03.ROM
Description for Customer :
	1. Modify BIOS for WLK 1.4.
==============================================================================
Model :	P55A01			FAB : 1.0		Author : Arcer Hwang
Old version : 979F1P03.BIN, 979F1P03.ROM
New version : 979F1P04.BIN(2MB for factory) Code Base : 02/20/2009	Build date : 10/30/2009
New version : 979F1P04.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 50A2(h) 979F1P04.BIN
CheckSum  : F03B(h) 979F1P04.ROM
Description for Customer :
	1. Update BIOS code for support Clarkdale C2 steping CPU(CPUID:20652).
==============================================================================
Model :	P55A01			FAB : 1.0		Author : Arcer Hwang
Old version : 979F1P04.BIN, 979F1P04.ROM
New version : 979F1P05.BIN(2MB for factory) Code Base : 02/20/2009	Build date : 11/25/2009
New version : 979F1P05.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : A4AE(h) 979F1P05.BIN
CheckSum  : 4447(h) 979F1P05.ROM
Description for Customer :
	1. Fixed Lynnfield 750 CPU(CPUID:106E5) show wrong core count.
	2. Fixed Clarkdale G9650 CPU(CPUID:20652) hang-up on BIOS CMOS setup CPU Configuration page.
	3. Fixed dale CPU PEG port can't run link x16 mode.
==============================================================================
Model :	P55A01			FAB : 1.0		Author : Arcer Hwang
Old version : 979F1P05.BIN, 979F1P05.ROM
New version : 979F1P06.BIN(2MB for factory) Code Base : 02/20/2009	Build date : 04/09/2010
New version : 979F1P06.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : C82A(h) 979F1P06.BIN
CheckSum  : 2568(h) 979F1P06.ROM
Description for Customer :
	1. Fixed USB port can't connect to iPhone.
	2. Update Ignition firmware from version 6.0.0.1126 to version 6.0.30.1199.
	3. Added support CPU i7-875K(Q3Z3),i5-655K(Q4MA),i7-880(Q3M5),i7-870S(Q3MT),i3-550(Q4DD).
==============================================================================
Model :	P55A01			FAB : 1.0		Author : Arcer Hwang
Old version : 979F1P06.BIN, 979F1P06.ROM
New version : 979F1P07.BIN(2MB for factory) Code Base : 02/20/2009	Build date : 05/11/2010
New version : 979F1P07.ROM(1MB for update BIOS utility FPT.EXE or FPTW.EXE)

LAN ROM	  : rtegpxe.lom
Raid BIOS : RAID_OR.BIN, 6121_Part1.BIN, 6121_Part2.BIN
CheckSum  : 85EF(h) 979F1P07.BIN
CheckSum  : E32D(h) 979F1P07.ROM
Description for Customer :
	1. Fixed CPU i7-875K(Q3Z3),i5-655K(Q4MA) OS blue screen issue.
	2. Update CPU microcode for CPUID 106E5(M13106E5_00000004.TXT).
==============================================================================